AK4356

DIGITAL AUDIO DACs
AK4356
192kHz 24-Bit 6ch DAC for DVD-Audio

28-pin VSOP
(5.6 9.8 1.2 mm)

1. 128x Oversampling
2. Sampling Rate up to 192kHz for 2 channels mode, 96kHz for 6 channels mode
3. 24-bit 8 times Digital Filter with Slow roll-off option
   • Ripple: ±0.005dB, Attenuation: 75dB
4. THD+N: ‚94dB
5. DR, S/N: 112dB
6. High Tolerance to Clock Jitter
7. Low Distortion Differential Output
8. Channel Independent Digital De-emphasis for 32, 44.1 & 48kHz sampling
9. Channel Independent Zero Detect Pin
10. Channel Independent Digital Attenuator with soft-transition
11. Soft Mute
12. 3-wire Serial Interface for Volume Control
13. I/F format: MSB justified, LSB justified, I2S
14. TTL Level Digital l/F
15. Master Clock
    • Normal Speed: 256fs, 384fs, 512fs or 768fs
    • Double Speed: 128fs, 192fs, 256fs or 384fs
16. Power Supply: 4.5 to 5.25V
17. 44-pin LQFP package
18. Ta: ‚40 to 85°C
19. Evaluation Board: AKD4356

PDF Download |  | Data Sheets Rev.M0072-E-02 2003/09 PDF : 293KB / 30pages |  | Evalution Board Manual Rev. KM060602 99/11 PDF : 298KB / 27pages

AK4356 BLOCK DIAGRAM